|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | min | Max | step |
| Current | 0.4 mA | 10 mA | 0.2mA |
| Frequency | 5 Hz | 50 Hz | 5 Hz |
| Pulse width | 1 % | 100% | 1% |
| Intermittent mode | | | |
| Number of cycles in intermittent mode | 2 | 40 | 1 |
| On cycle time | 10 sec | 120 sec | 1 sec |
| OFF cycle time | 10 sec | 120 sec | 1 sec |
| Single cycle mode | | | |
| Stimulation time | 5 min | 60 min | 1 min |
|  |  |  |  |

Current: unipolar (positive or negative) and bipolar

Sham: yes

Types of stimulations: Single cycle, intermittent