**Sensitive Electrochemical Determination of Hydrogen Peroxide using Copper Nanoparticles in a Polyaniline Film on a Glassy Carbon Electrode**

**Jing Lianga, Maochao Weia, Qiang Wangb, Zongshan Zhaoa,\*, Aifeng Liua, Zhuanni Yu,b and Yong Tian****a**

aCAS Key Laboratory of Biobased Materials, Qingdao Institute of Bioenergy and Bioprocess Technology, Chinese Academy of Sciences, Qingdao 266101, China.

b College of Chemistry and Pharmaceutical Sciences, Qingdao Agricultural University, Qingdao 266109, China.

\*Corresponding author. Fax/Tel: +86 532-80662709, E-mail: [zhaozs@qibebt.ac.cn](https://mail.cstnet.cn/coremail/XJS/pab/view.jsp?sid=BAiXtmqqertBMmFVXPqqSICRZrqHsKxY&totalCount=6&view_no=5&puid=1&gid=COWORKERS).

**SUPPLEMENTARY MATERIAL**


****

Figure S1. Fourier transform infrared spectra of polyaniline and polyaniline/Cu particles


****

Figure S2. Cyclic voltammograms and plot of peak current versus scan rate.of H2O2 (0.1 M ) on polyaniline electrode (A, B) in buffer (pH 6.5) and polyaniline/Cu electrode (C, D) in H2O2 solution at scan rates of 10, 50, 100, 150, 200, 250 and 300 mV/s, respectively.




Figure S3. Influence of the potential co-existing species on polyaniline/Cu electrode.


****

Figure S4. Amperometric responses of polyaniline/Cu electrode for detecting H2O2 in tap water samples