Additional file for:

Application of biochar-coated urea controlled loss of fertilizer nitrogen and increased nitrogen use efficiency

Yiman Jiaa, Zhengyi Hua,b,c,\*, Yuxin Bad, wenfang Qie

a College of Resources and Environment, University of Chinese Academy of Sciences, Beijing 101408, China

b Sino- Danish Center for Education and Research, Beijing 100190, China

c Research Center for Eco-Environmental Sciences, Chinese Academy of Sciences, Beijing 100085, China

d Blue Sky Zhenggao (Beijing) Agricultural Science and Technology Co., LTD


e Shenwu technology group corp Co., Ltd.

Corresponding author:


Zhengyi Hu

College of Resources and Environment, University of Chinese Academy of Sciences, Beijing 101408, China

E-mail: [zhyhu@ucas.ac.cn](mailto:zhyhu@ucas.ac.cn)




**Fig. S.1** SEM images of biochar used for biochar-coated urea.



**Fig. S.2** FTIR spectra of biochar used for biochar-coated urea.


The band at 1570 cm−1 correspond to keto C=O stretching vibrations in esters or C=C stretching vibrations in alkene and aromatic compounds;

The band at 1030 cm−1 correspond to C–O stretching vibrations in lignin derivatives or alcohols and phenols.”



**Fig. S.3** 13C NMR spectra of biochar used for biochar-coated urea.

Resonance region at 110–150 ppm indicated aromatic carbon.



**Fig. S.4** Schematic plot of ammonia volatilization collection.