Here is the instantiated security case for ACAS Xu (Airborne Collision Avoidance System Xu) represented in a hierarchical tree format using dashes (-) to denote different levels:

```

G0: ACAS Xu (Airborne Collision Avoidance System Xu) satisfies security requirements

- C0: ACAS Xu is a collision avoidance system designed for UAVs

- C1: Security requirements are requirements about protecting the system from malicious entities

- J0: The argumentation is based on satisfaction of security requirements

- A0: System security requirements are complete, adequate, and consistent

- S0: Argue through asset protection and secure development requirements

- G1: ACAS Xu satisfies the asset protection requirements

- A1: Asset inventory is established

- S1: Argue through the different stages of the system development life cycle

- G3: Asset protection requirements are met during the architecture design phase

- C2: ACAS Xu's architecture includes components like Sensors, Processor, Planner, and Actuator

- S2: Argue through derivating security threats from security requirements

- G5: ACAS Xu architecture is protected against identified security threats

- A2: All relevant threats have been identified

- S3: Argue over each security threat

- G0.1: ACAS Xu architecture is protected against ST1 (Tampering)

- G0.2: ACAS Xu architecture is protected against ST2 (Spoofing)

- G0.3: ACAS Xu architecture is protected against ST3 (Elevation of privileges)

- G4: Asset protection requirements are met during other phases (undevelopment)

- G2: ACAS Xu satisfies secure development requirements (undevelopment)

- G6: ACAS Xu architecture is validated (undevelopment)

- C3: ACAS Xu architecture model is well defined in a formal method

- A3: ACAS Xu architecture model is well defined in a formal method

- J1: Detection and mitigation of threats fulfill security requirements

```

Notice how the placeholders and decorators for uninstantiated, choice, multiplicity, and optionality have been removed and replaced with concrete information specific to ACAS Xu. Also, undeveloped nodes remain marked for further development.