Table 6: Recommended illumination levels for offices (Ruffles, 2009)

|  |  |
| --- | --- |
| Area | Recommended Lighting Level (Ix) |
| General | 500 |
| Computer Workstations | 300-500 |
| Filing Rooms | 300 |
| Print Rooms | 300 |
| Drawing Office | 500 |
| Drawing Boards | 750 |
| CAD Design Areas | 300-500 |