Table 8: Dependent and independent variables

|  |  |  |  |
| --- | --- | --- | --- |
| *Independent variables* | *Fixed independent variables* | Window- to-wall ratio | 90% |
| Window dimensions | 3.8m \* 2.8m |
| Motif dimensions | 0.38m \* 0.28m |
| Motif depth | 0.1 m |
| ***Non-fixed independent variables*** | **Opening ratio (OR) (indicating thickness)** | 30%, 50% and 70% |
| **Depth direction** | straightforward, downward (D), east (E) and west (W) |
| **Depth angle** | 30°,45° and 90° |
| *dependent* variables | * Useful daylight illuminance (UDI) - Target: 300 lux acceptable/ 500 lux preferred * Spatial Daylight Autonomy (sDA) - ASE <10% * Annual Sunlight Exposure (ASE) - >55% - 2 points on LEED, >75% - 3 points on LEED | | |